For 1990-2009 cars

## Power Steering Fluid Reservoir Replacement - Off Vehicle L61

### Removal Procedure

1. Remove the power steering pump assembly. Refer to Power Steering Pump Replacement .
2. Remove the pump to reservoir retaining clips. Discard the clips.
3. Carefully remove the reservoir from the pump housing.
4. Remove the O-ring from the pump housing. Discard the O-ring.

### Installation Procedure

Important: Lubricate the O-ring using clean power steering fluid.

1. Install a new O-ring.

Important: The reservoir must pushed straight onto the pump housing.

2. Install the reservoir to the pump housing. Refer to Power Steering Pump Replacement .
3. Install new pump to reservoir retaining clips.
4. Install the power steering pump assembly. Refer to Power Steering Pump Replacement .

.