For 1990-2009 cars

### Removal Procedure

1. Remove the fog lamp. Refer to Front Fog Lamp Replacement .
2. Depress the inboard bezel to front fascia retainer tab.
3. Remove the bezel from the front fascia by tilting outward.

### Installation Procedure

1. Position the bezel to the front fascia.
2. Install the bezel, pressing into place until fully seated.
3. Install the fog lamp. Refer to Front Fog Lamp Replacement .