For 1990-2009 cars

#### Tools Required

J 38122-A Harmonic Balancer Holder

### Removal Procedure

1. Install the J 38122-A onto the damper assembly.
2. Remove and discard the damper retaining bolt and washer. Use the J 38122-A and breaker bar in order to prevent the crankshaft from rotating when loosening the bolt.
3. Remove the damper assembly.

### Installation Procedure

1. Lubricate the front oil seal and seal surface of the crankshaft balancer with an engine oil supplement.

Notice: Misalignment of the keyway may cause damage to the oil pump.

2. Install the damper onto the crankshaft indexing keyway. Use care to properly align the keyway and flats on the damper with the oil pump drive.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the new retaining bolt and washer using the J 38122-A and a breaker bar to hold the crankshaft.

Tighten
Tighten the crankshaft pulley bolt to 100 N·m (74 lb ft) plus 75 degrees.