For 1990-2009 cars

### Removal Procedure

Left front door shown. The rest of the doors are similar.

1. Remove the screw (1).
2. Remove the switch from the door pillar.

May need to pry the switch out with a flat-bladed tool.

3. Disconnect the wire harness.

### Installation Procedure

1. Install the connector to the switch.
2. Install the switch

Notice: Refer to Fastener Notice in the Preface section.

3. Install the screw (1).

Tighten
Tighten the screw (1) to 2 N·m (18 lb in).