For 1990-2009 cars

#### Tools Required

J 44723 Transmission/Stand Adapter Plate

Caution: The torque converter must be held to the torque converter housing by a retaining device such as shipping brackets. Without the retaining device, the torque converter may slide forward, disengaging the oil pump, or may fall completely out of the transmission causing personal injury and/or property damage.

Caution: The 1000 Series™ transmission dry weight is approximately 150 kg (330 lb). To help avoid personal injury and/or property damage: Use caution when installing, removing, or moving the transmission. Get help when lifting the transmission. Assistance from a hoist or another person may be required. Ensure that lifting equipment can properly support the transmission.

1. Position the transmission on the work table so that it is resting on the oil pan.
2. Remove 12 power take-off (PTO) cover bolts (3)
3. Remove 2 PTO covers (2).
4. Remove the PTO gaskets (1).
5. Install J 44723 onto the repair stand.
6. Attach a sling to the transmission.
7. Attach a hoist to the sling.
8. Raise the transmission to adapter plate J 44723 .

Caution: If the transmission is not secured properly to the adapter plate, the transmission could fall. To help avoid personal injury and/or property damage: Use at least 5 bolts to support the transmission. Use M10 x 1.5 bolts with 19-25 mm (3/4-1 inch) thread engagement. If the proper bolt is not used, the PTO bolt holes may be damaged.

9. Secure the transmission to J 44723 using either of the PTO mounting pads as the attachment point.
10. Remove the sling from the transmission.