For 1990-2009 cars

### Removal Procedure

1. Open the rear door.
2. Pull back the roof rail weatherstrip.
3. Pull back the rear door opening weatherstrip.
4. Remove the screws from the C-pillar applique.
5. Remove the C-pillar applique by prying up from the door opening side and then rearward to detach the adhesive strips.
6. Clean the adhesive strips from the door opening and the applique.

### Installation Procedure

1. Install new adhesive strips to the C-pillar.
2. Position the applique to the screw holes in the C-pillar.
3. Install the applique to the C-pillar pressing into place until seated.

Notice: Refer to Fastener Notice in the Preface section.

4. Install the screws to the applique.

Tighten
Tighten the screws to 3 N·m (27 lb in).

5. Install the roof rail weatherstrip.
6. Install the rear door opening weatherstrip.
7. Close the door .
8. Inspect the rear door weatherstrips fro proper fit and alignment.