For 1990-2009 cars

### Removal Procedure

1. Remove the rear bumper fascia. Refer to Rear Bumper Fascia Replacement .
2. Remove the push-in retainers from the rear bumper energy absorber.
3. Remove the energy absorber from the rear bumper impact bar.

### Installation Procedure

1. Position the energy absorber to the rear bumper impact bar.
2. Install the push-in retainers to the rear bumper energy absorber.
3. Install the rear bumper fascia. Refer to Rear Bumper Fascia Replacement .