For 1990-2009 cars

#### Tools Required

KM-906-B Bushing Remover/Installer Kit

### Removal Procedure

1. Remove the rear support assembly. Refer to Support Replacement .
2. Using the KM-906-B , install the KM-906-70, KM-906-11 and KM-906-12A in order to press out the rear suspension support bushings.
3. Remove the KM-906-70, KM-906-11 and KM-906-12A with the bushing.

### Installation Procedure

1. Using the KM-906-B , assemble the KM-906-70, KM-906-13A and KM-906-14 with the new bushing in order to install the new bushing.
2. Remove the KM-906-70, KM-906-13A and KM-906-14.
3. Install the rear support assembly. Refer to Support Replacement .