For 1990-2009 cars

### Removal Procedure

1. Remove the lift gate pull handle. Refer to Liftgate Pull Strap Replacement .
2. Remove the lift gate trim panel retainers.
3. Remove the trim panel.

### Installation Procedure

1. Position the trim panel to the lift gate.
2. Secure the trim panel to the structure by pushing in at the retainer locations.
3. Install the trim panel retainers.
4. Install the lift gate pull handle. Refer to Liftgate Pull Strap Replacement .