For 1990-2009 cars

## Rear Door Frame Applique Replacement Sedan /Wagon

### Removal Procedure

1. Remove the rear door outer belt seal. Refer to Rear Door Window Belt Outer Sealing Strip Replacement .
2. Slide the applique up.
3. Remove the applique by tilt the front edge out evenly and pull out from the door window frame.

### Installation Procedure

1. Position the applique to the slots in the rear door window frame.
2. Slide the applique into the slots , moving slightly forward and down.
3. Install the rear door outer belt seal. Refer to Rear Door Window Belt Outer Sealing Strip Replacement .

## Rear Door Frame Applique Replacement Sedan/Wagon

### Removal Procedure

1. Remove the rear door outer belt seal. Refer to Rear Door Window Belt Outer Sealing Strip Replacement .
2. Remove the fastener from the applique.
3. Slide the applique up.
4. Remove the applique by tilt the front edge out evenly and pull out from the door window frame.

### Installation Procedure

1. Position the applique to the slots in the rear door window frame.
2. Slide the applique into the slots and move slightly forward and down.
3. Install the push-in retainer to the applique.
4. Install the rear door outer belt seal. Refer to Rear Door Window Belt Outer Sealing Strip Replacement .