For 1990-2009 cars

## Power Steering Return Hose Replacement L61

### Removal Procedure

1. Remove the power steering reservoir cap.
2. Disconnect the power steering return hose from the steering gear.
3. Disconnect the power steering return hose from the reservoir.
4. Separate the power steering return hose from the power steering pressure hose. Note the hose routing for installation.
5. Remove the power steering return hose from the vehicle.

### Installation Procedure

1. Position the power steering return hose as noted during removal.

Notice: Refer to Fastener Notice in the Preface section.

2. Connect the power steering return hose to power steering gear.

Tighten
Tighten the fitting to 27 N·m (20 lb ft).

3. Connect the power steering return hose to the reservoir.

Tighten
Tighten the clamp to 2.5 N·m (22 lb in).

4. Fill and bleed the power steering system. Refer to Power Steering System Bleeding .