For 1990-2009 cars

Table 1: | Capacities
Table 2: | Specifications

The following approximate capacities are given in English and metric conversions.

#### Capacities

Fluid Changes | Capacities
--- | ---
Manual Transaxle | 2.0 quarts (1.9 L)
Automatic Transaxle | 6.9 quarts (6.5 L)
Cooling System | -
2.2L L4 (L61) Engine (Manual Transaxle) | 7.4 quarts (7.0 L)
2.2L L4 (L61) Engine (Automatic Transaxle) | 7.3 quarts (7.0 L)
3.0L V6 (L81) Engine | 8.5 quarts (8.0 L)
2.2L L4 (L61) Engine Crankcase (with Filter Change) | 5.0 quarts (4.7 L)
3.0L V6 (L81) Engine Crankcase (with Filter Change) | 5.0 quarts (4.7 L)
Fuel Tank | 15.7 gallons (59.4 L)
Power Steering -- 2.2L L4 Engine | -
Pump Only | 17 ounces (0.5 L)
Complete System | 23 ounces (0.7 L)
Power Steering -- 3.0L V6 (L81) Engine | -
Pump Only | 10 ounces (0.3 L)
Complete System | 23 ounces (0.7 L)
Windshield Washer Solvent (Container) | 2.08 quarts 1.97 L
NOTE: All capacities are approximate. When adding, be sure to fill to the approximate level, as recommended in this manual. Recheck fluid level after filling.

#### Specifications

Engine Type | 2.2L L4 Engine (L61); 3.0L V6 Engine (L81)
Engine Firing Order |
2.2.L L4 (L61) Engine | 1-3-4-2
3.0L V6 (L81) Engine | 1-2-3-4-5-6
Thermostat Temperature | 194°F (90°C)
Wheel Nut Torque | 125 N·m 92 ft lb
Tire Pressures and Sizes: See the Tire Loading Information Label, located on the rear edge of the driver's side rear door.