For 1990-2009 cars

## Radiator Outlet Hose Replacement L61

### Removal Procedure

1. Remove the battery. Refer to Battery Replacement in Engine Electrical.
2. Drain the coolant. Refer to Cooling System Draining and Filling .
3. Remove the clamp which secures the lower radiator hose to the engine block.
4. Remove the lower radiator hose from the engine block.
5. Remove the clamp which secures the return hose to the surge tank.
6. Remove the return hose from the surge tank.
7. Remove the clamp which secures the lower radiator hose to the radiator.
8. Remove the lower radiator hose from the radiator.
9. Remove the clamp which secures the lower radiator hose to the engine bracket.
10. Remove the lower radiator hose.

### Installation Procedure

Important: The white line on the hose should be installed at the 12 o'clock position.

1. Position the lower radiator hose into the engine bracket clamp.
2. Install the lower radiator hose to the engine block.
3. Install the lower radiator hose clamp to the 1 o'clock position.
4. Install the return hose to the surge tank.
5. Install the return hose clamp to the 2 o'clock position.

Important: The white line on the hose should be installed at the 12 o'clock position.

6. Install the lower radiator hose to radiator outlet.
7. Install the lower radiator hose clamp to the 12 o'clock position.
8. Secure the lower radiator hose into the engine bracket clamp.
9. Install the battery. Refer to Battery Replacement in Engine Electrical.
10. Fill the coolant. Refer to Cooling System Draining and Filling .

## Radiator Outlet Hose Replacement L81

### Removal Procedure

1. Remove the battery. Refer to Battery Replacement in Engine Electrical.
2. Drain the coolant. Refer to Cooling System Draining and Filling .
3. Remove the clamp which secures the lower radiator hose to the engine block.
4. Remove the lower radiator hose from the engine block.
5. Remove the upper transaxle cooler line from the radiator.
6. Remove the lower radiator hose clamp.
7. Remove the lower radiator hose from the radiator.
8. Remove the clamp which secures the lower radiator hose to the wiring harness.

### Installation Procedure

1. Install the lower radiator hose to the engine block fitting.

Important: The white line on the hose should be installed at the 12 o'clock position.

2. Install the lower radiator hose clamp at the 1 o'clock position.
3. Install the lower radiator hose to the radiator.

Important: The white line on the hose should be installed at the 12 o'clock position.

4. Install the lower radiator hose clamp at the 11 o'clock position.
5. Install the lower radiator hose into the wiring harness clamp.
6. Install the outlet hose to the radiator.
7. Install the outlet hose clamp at the 12 o'clock position.
8. Install the upper transaxle cooler line to the radiator end tank.

Tighten
Tighten the cooler line to 25 N·m (18 lb ft).

9. Install the battery. Refer to Battery Replacement in Engine Electrical .
10. Install the fan control module by sliding down onto the bracket.
11. Fill the cooling system. Refer to Cooling System Draining and Filling .