For 1990-2009 cars

### Removal Procedure

1. Disable the SIR system. Refer to "Disabling SIR System" in this service manual.
2. Remove the automatic transaxle control assembly. Refer to "Automatic Transaxle Control Assembly Removal" in this service manual.
3. Using an electrical terminal pick, remove the solenoid electrical terminals from the connector body.
4. Using a 5/32 in. drill bit, drill out the rivet attaching the solenoid to control assembly.
5. Remove the shift lock control solenoid.

### Installation Procedure

1. Route the shift lock control solenoid wires through the opening in the control assembly.
2. Insert the wire terminals into the connector body.
3. Position the solenoid to control assembly and install the solenoid pop rivet with a rivet gun.
4. Install the automatic transaxle control assembly. Refer to "Automatic Transaxle Control Assembly Installation" in this service manual.
5. Enable the SIR system. Refer to "Enabling SIR System" in this service manual.