For 1990-2009 cars

### Removal Procedure

Caution: When a hood hold open device is being removed or installed, provide alternate support to avoid the possibility of damage to the vehicle or personal injury.

1. Open the hood and support with the appropriate auxiliary prop device.
2. Remove the screws from the prop rod bracket and remove the prop rod.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the prop rod bracket and screws.

Tighten
Tighten the screws to 8 N·m (71 lb in).

2. Remove the auxiliary prop device.
3. Close the hood.