For 1990-2009 cars

## Output Speed Sensor Installation 2WD

#### Tools Required

J 36850 Transjel® Lubricant

1. Install the vehicle speed sensor O-ring (3) onto the output speed sensor (OSS) (2).
2. Apply J 36850 to the O-ring (3).
3. Install the OSS (2) into the low and reverse clutch housing, 2WD.

Notice: Refer to Fastener Notice in the Preface section.

4. Install the vehicle speed sensor bolt (1) into the low and reverse clutch housing, 2WD.

Tighten
Tighten the bolt to 12 N·m (108 lb in).