For 1990-2009 cars

### Removal Procedure

1. Remove the outer trim panel from the seat cushion. Refer to Front Seat Front Finish Panel Replacement .
2. Disconnect the electrical connector from the switch.
3. Using a small flat-bladed tool, pry the power seat switch from the side trim.

### Installation Procedure

1. Install the power seat switch to the trim panel.
2. Connect the electrical connector to the switch.
3. Install the outer trim panel to the seat cushion. Refer to Front Seat Front Finish Panel Replacement .