For 1990-2009 cars

### Removal Procedure

1. Remove the rear support assembly. Refer to Support Replacement .
2. Remove the rear suspension upper control arm to support assembly bolt and nut. Discard the nut and bolt.
3. Remove the rear suspension upper control arm from the support assembly.

### Installation Procedure

1. Install the rear suspension upper control arm to the support assembly.

Notice: Refer to Fastener Notice in the Preface section.

2. Install a new nut and bolt to the rear suspension upper control arm to support assembly.

Tighten
Tighten the nut and bolt to 90 N·m (66 lb ft) plus and additional 60 to 75 degrees.

3. Install the rear support assembly. Refer to Support Replacement .