For 1990-2009 cars

### Removal Procedure

1. Move the front seat to the forward most position.
2. Remove the carpet retainer in the area surrounding the center pillar lower molding by pulling at the attaching clip locations.
3. Install the masking tape around the center pillar at the lower portion of the upper molding to ensure that the upper molding stays attached to the center pillar.

### Installation Procedure

1. Engage the center pillar lower attaching tabs to the center pillar upper molding.
2. Secure the center pillar lower molding to the vehicle by gently pushing on the molding at the attaching clip locations.
3. Remove the tape.
4. Install the carpet retainer by gently pushing at the attaching clip locations.
5. Install the weatherstrip over the center pillar lower molding and the carpet retainer using a flat-blade tool.
6. Function the shoulder belt to ensure the proper operation.
7. Place the front seat in the original position.