For 1990-2009 cars

## Diagnostic System Check - Cruise Control L81

### Test Description

The numbers below refer to the step numbers on the diagnostic table.

1. Lack of communication may be due to a malfunction in the Keyword or the class 2 serial data circuit. The specified procedure will determine the particular condition.

2. The presence of DTCs which begin with U indicates that some other module is not communicating. The specified procedure will compile all the available information before tests are performed.

Step | Action | Yes | No
--- | --- | --- | ---
1 | Install a scan tool. Does the scan tool power up? | Go to Step 2 | Go to Scan Tool Does Not Power Up in Data Link Communications
2 |

1. Turn the ignition ON, with the engine OFF.
2. Attempt to establish communication with the following modules:

• | Engine control module (ECM)

• | Electronic brake control module (EBCM)

Does the scan tool communicate with the modules listed above?

Go to Step 3

Go to Scan Tool Does Not Communicate with Class 2 Device or Scan Tool Does Not Communicate with Keyword Data Line in Data Link Communications

3 | Select the DTCs function on the scan tool for the following modules:

• | ECM

• | EBCM

Does the scan tool display any DTCs for the modules listed above?

Go to Step 4

Go to Symptoms - Cruise Control

4 | Does the scan tool display any DTCs which begin with a "U"? | Go to Diagnostic Trouble Code (DTC) List in Data Link Communications | Go to Step 5
5 | Does the scan tool display DTC P0560, P2500 or P2501? | Go to Diagnostic Trouble Code (DTC) List in Engine Electrical | Go to Diagnostic Trouble Code (DTC) List

## Diagnostic System Check - Cruise Control L61

### Test Description

The numbers below refer to the step numbers on the diagnostic table.

1. Lack of communication may be due to a partial malfunction of the class 2 serial data circuit or due to a total malfunction of the class 2 serial data circuit. The specified procedure will determine the particular condition.

2. The symptom list in Symptoms will determine the correct diagnostic procedure to use.

Step | Action | Yes | No
--- | --- | --- | ---
1 | Install a scan tool. Does the scan tool power up? | Go to Step 2 | Go to Scan Tool Does Not Power Up in Data Link Communications
2 |

1. Turn ON the ignition, with the engine OFF.
2. Attempt to establish communication with the Powertrain Control Module (PCM) and Electronic Brake Control Module (EBCM).

Does the scan tool communicate with the control modules?

Go to Step 3

Go to Scan Tool Does Not Communicate with Class 2 Device in Data Link Communications

3 | Select the PCM display DTC function on the scan tool. Does the scan tool display any DTCs? | Go to Diagnostic Trouble Code (DTC) List in Engine Controls-2.2L | Go to Step 4
4 | Select the EBCM display DTC function on the scan tool. Does the scan tool display any DTCs? | Go to Diagnostic Trouble Code (DTC) List in Antilock Brake System | Go to Symptoms - Cruise Control