For 1990-2009 cars

## Transmission Range Switch Logic 2.2L

#### Transmission Range Switch Logic-2.2L (L61)

Gear Selector Position | Signal A | Signal B | Signal C | Signal P
--- | --- | --- | --- | ---
Park (P) | LOW | HI | HI | LOW
Reverse (R) | LOW | LOW | HI | HI
Neutral (N) | HI | LOW | HI | LOW
Drive 4 (OD) | HI | LOW | LOW | HI
Drive 3 (3) | LOW | LOW | LOW | LOW
Drive 2 (2) | LOW | HI | LOW | HI
Drive 1 (1) | HI | HI | LOW | LOW
HI = Ignition voltage LOW = 0 volts

## Transmission Range Switch Logic 3.0L

#### Transmission Range Switch Logic-3.0L (L81)

Gear Selector Position | Signal A | Signal B | Signal C | Signal P
--- | --- | --- | --- | ---
Park (P) | HI | LOW | LOW | HI
Reverse (R) | HI | HI | LOW | LOW
Neutral (N) | LOW | HI | LOW | HI
Drive 4 (OD) | LOW | HI | HI | LOW
Drive 3 (3) | HI | HI | HI | HI
Drive 2 (2) | HI | LOW | HI | LOW
Drive 1 (1) | LOW | LOW | HI | HI
HI = Ignition voltage LOW = 0 volts