For 1990-2009 cars

#### Tools Required

J 44020 Terminal Repair Kit

The Supplemental Inflatable Restraint (SIR) System/Supplemental Restraint System (SRS) requires special wiring repair procedures due to the sensitive nature of the circuitry. Follow the specific procedures and instructions when working with the SIR/SRS system wiring, and the wiring components, such as connectors and terminals.

### SIR/SRS Connector (Plastic Body and Terminal Metal Pin) Repair

Use the connector and wire repair assembly packs, available through Saturn Service Parts, to repair the damaged SIR/SRS wire harness connectors and the terminals. These kits include an instruction sheet and the DuraSeal spliced sleeves. Use the DuraSeal splice sleeves in order to splice the new wires, connectors, and terminals to the harness. The splice crimping tool is color keyed in order to match the splices from J 44020 . You must use the splice crimping tool in order to apply these splices.

If the individual terminals are damaged on the sensing and diagnostic module (SDM) harness connector, use 1 of the following 2 components in order to replace the SDM harness connector:

• | The SDM harness connector pigtail assembly

• | The SDM harness connector replacement kit

If the individual terminals are damaged on any other SIR/SRS connection, use the appropriate connector repair assembly pack in order to replace the entire connection. Replace the entire SIR/SRS wiring harness, if needed, in order to maintain SIR/SRS circuit integrity.

### SIR/SRS Wire Pigtail Repair

Important: Do not make wire, connector, or terminal repairs on components with wire pigtails.

A wire pigtail is a wire or wires attached directly to the device, not by a connector. If a wiring pigtail is damaged, you must replace the entire component, with pigtail. The inflatable restraint steering wheel module coil is an example of a pigtail component.

### SIR/SRS Wire Repair

Important: Refer to Wiring Repairs in order to determine the correct wire size for the circuit you are repairing. You must obtain this information in order to ensure circuit integrity.

If any wire except the pigtail is damaged, repair the wire by splicing in a new section of wire. Use the DuraSeal splice sleeves and splice crimping tool from the J 44020 . Use the following wiring repair procedures in order to ensure the integrity of the DuraSeal splice sleeves.

Splice Sleeve Color | Crimp Tool Nest Color | Wire Gage mm² / (AWG)
--- | --- | ---
Salmon (Yellow-Pink) 12089189 | Red (1) | 0.035-0.8 / (18-20)
Blue 12089190 | Blue (2) | 1.0-2.0 / (14-16)
Yellow 12089191 | Yellow (3) | 3.0-5.0 / (10-12)
Green 88988379 | Red (1) | 0.22-0.35 / (22-24)

Important: You must perform the following procedures in the listed order. Repeat the procedure if any wire strands are damaged. You must obtain a clean strip with all of the wire strands intact.

1. Open the harness by removing any tape:

• | Use a sewing seam ripper, available from sewing supply stores, in order to cut open the harness in order to avoid wire insulation damage.

• | Use the DuraSeal splice sleeves on all types of insulation except tefzel and coaxial.

• | Do not use the DuraSeal splice sleeve to form a splice with more than 2 wires coming together.

2. Cut as little wire off the harness as possible. You may need the extra length of wire in order to change the location of a splice.

Adjust splice locations so that each splice is at least 40 mm (1.5 in) away from the other splices, harness branches, or connectors.

3. Strip the insulation:

• | Perform one of the following items in order to find the correct wire size:

- | Find the wire on the schematic and convert the metric size to the equivalent AWG size.

- | Use an AWG wire gage.

- | If you are unsure of the wire size, begin with the largest opening in the wire stripper and work down until achieving a clean strip of the insulation.

• | Strip approximately 7.5 mm (0.313 in) of insulation from each wire to be spliced.

• | Do not nick or cut any of the strands. Inspect the stripped wire for nicks or cut strands.

• | If the wire is damaged, repeat this procedure after removing the damaged section.

4. Select the proper DuraSeal splice sleeve according to the wire size. Refer to the above table at the beginning of the repair procedure for the color coding of the DuraSeal splice sleeves and the crimp tool nests.
5. Use the splice crimp tool from the J 44020 to crimp the DuraSeal splice sleeves. In order to position the DuraSeal splice sleeve in the proper color nest of the splice crimp tool.

The crimp tool has 3 nests, 1 is for the salmon and green splice sleeves, 2 is for the blue splice sleeves and 3 is for the yellow splice sleeves.

6. Place the DuraSeal splice sleeve in the nest. Ensure that the crimp falls midway between the end of the barrel and the stop. The sleeve has a stop (3) in the middle of the barrel (2) in order to prevent the wire (1) from going further. Close the hand crimper handles slightly in order to firmly hold the DuraSeal splice sleeve in the proper nest.
7. Insert the wire into the DuraSeal splice sleeve barrel until the wire hits the barrel stop.
8. Tightly close the handles of the crimp tool until the crimper handles open when released.

The crimper handles will not open until you apply the proper amount of pressure to the DuraSeal splice sleeve. Repeat steps 4 and 5 for the opposite end of the splice.

9. Using the heat torch, apply heat to the crimped area of the barrel.
10. Gradually move the heat barrel to the open end of the tubing:

• | The tubing will shrink completely as the heat is moved along the insulation.

• | A small amount of sealant will come out of the end of the tubing when sufficient shrinkage is achieved.

### Connector Position Assurance (CPA)

The connector position assurance (CPA) is a small plastic insert that fits through the locking tabs of a connector. CPAs are used in all SIR system connectors and also in some connectors of other systems. The CPA ensures that the connector halves cannot vibrate apart. You must have the CPA in place in order to ensure good contact between the mating terminals of a connection.

### Terminal Position Assurance (TPA)

The terminal position assurance (TPA) insert resembles the plastic combs used in the control module connectors. The TPA keeps the terminal securely seated in the connector body. Do not remove the TPA from the connector body unless you remove a terminal for replacement.