For 1990-2009 cars

### Removal Procedure

Caution: When a hood hold open device is being removed or installed, provide alternate support to avoid the possibility of damage to the vehicle or personal injury.

1. Open and support the hood.
2. Mark the position of the hood hinge by marking around the hood hinges with a grease pencil.
3. Remove the hood. Refer to Hood Replacement .
4. Remove the hinge bolts from the hinge.
5. Remove the hinge from the vehicle.

### Installation Procedure

1. Position the hinge to the vehicle and align the hinge to the locating marks.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the bolts to the hinge.

Tighten
Tighten the bolts to 20 N·m (15 lb ft).

3. Install the hood. Refer to Hood Replacement .
4. Close the hood.