For 1990-2009 cars

Scan Tool Output Control | Additional Menu Selection(s) | Description
--- | --- | ---
ABS Warning Lamp | Lamp Tests | Commands the ABS indicator ON and OFF.
Automated Bleed Procedure | Automated Bleed | Used in order to bleed the ABS hydraulics.
Automated Test Procedure | Automated Test | Used in order to activate the ABS solenoids and pump motor.
LF Inlet Valve Solenoid | Solenoid Test | Commands the solenoid ON and OFF.
LF Outlet Valve Solenoid | Solenoid Test | Commands the solenoid ON and OFF.
Low Traction Lamp | Lamp Tests | Commands the Low Traction Lamp ON and OFF.
LR Inlet Valve Solenoid | Solenoid Test | Commands the solenoid ON and OFF.
LR Outlet Valve Solenoid | Solenoid Test | Commands the solenoid ON and OFF.
RF Inlet Valve Solenoid | Solenoid Test | Commands the solenoid ON and OFF.
RF Outlet Valve Solenoid | Solenoid Test | Commands the solenoid ON and OFF.
RR Inlet Valve Solenoid | Solenoid Test | Commands the solenoid ON and OFF.
RR Outlet Valve Solenoid | Solenoid Test | Commands the solenoid ON and OFF.