For 1990-2009 cars

#### Tools Required

• | J 22828 Input and Countershaft Race Installer

• | J 24433 Press Tube

Important:

• | Lubricate all components in transmission fluid before installation.

• | Make sure the oil hole in the collar is 90 degrees from the oil hole in the output shaft.

1. Install the thrust washer using the J 24433 and a hydraulic press.
2. Install the collar using the J 24433 and a hydraulic press.
3. Install the caged needle bearings (3).
4. Install the reverse gear (2).
5. Install the reverse gear blocking ring (1).

Important:

• | The raised center hub of the 5th/Reverse synchronizer assembly faces the 5th gear.

• | Line up the blocking ring tabs and the hub keyways while pressing.

6. Install the 5th/Reverse synchronizer using the J 24433 and a hydraulic press.
7. Install the bearing collar using an appropriate tool and a hydraulic press.
8. Install the 5th gear blocking ring (3).
9. Install the two caged needle bearings (2).
10. Install the 5th gear (1).

Important: The 3rd gear will install very tight, press load may exceed some press limitations. Ensure that the mating surfaces are clean.

11. Install the 3rd gear using the J 22828 and a hydraulic press.

Important: The 4th gear will install very tight, press load may exceed some press limitations. Ensure that the mating surfaces are clean.

12. Install the 4th gear using the J 22828 and a hydraulic press.