For 1990-2009 cars

1. Check the end play between the intermediate carrier assembly (1) and the thrust washer (2) at each pinion gear (3).
2. If the end play exceeds specifications replace the intermediate carrier assembly.

Specification
The maximum end play is 1.01 mm (0.040 in).

3. Inspect the bushing (1) for wear and damage.
4. Measure the inside diameter (ID) of the bushing at dimension A.
5. If the bushing ID exceeds specifications, replace the bushing.

Specification
The bushing maximum ID is 36.575 mm (1.4400 in)