For 1990-2009 cars

### Removal Procedure

1. Drain the washer solvent from the washer solvent container.
2. Remove the right front fender liner. Refer to Front Wheelhouse Liner Replacement in Body Front End.
3. Disconnect the washer solvent container level sensor electrical connector.
4. Using a small flat-bladed tool, remove the washer solvent level sensor from the washer solvent container.
5. Using a small flat-bladed tool, remove the seal from the washer solvent container.

### Installation Procedure

1. Position the seal to the washer solvent container, pressing in until fully seated.
2. Position the washer solvent level sensor to the washer solvent container, pressing in until fully seated.
3. Connect the washer solvent level sensor electrical connector.
4. Install the right front fender liner. Refer to Front Wheelhouse Liner Replacement in Body Front End.
5. Fill the washer solvent container with washer solvent .