For 1990-2009 cars

### Removal Procedure

1. Remove the rear washer nozzle grommet.
2. Apply tape around base of the nozzle on the lift gate to protect the paint.
3. Use small flat-bladed tool to depress the washer nozzle tabs while pulling outward.
4. Disconnect the rear washer nozzle hose and remove the washer nozzle.

### Installation Procedure

1. Connect the rear washer nozzle hose.
2. Install the rear washer nozzle hose to the lift gate.
3. Install the rear washer nozzle grommet.
4. Remove the tape from vehicle.