For 1990-2009 cars

### Disassembly Procedure

1. Remove the Steering Wheel. Refer to Steering Wheel Replacement
2. Remove the screws from the steering wheel shroud

Notice: Cruise control switches must be removed from the rear. Do not attempt to pry them out from front as damage to steering wheel may occur.

3. If the vehicle is equipped with cruise control, push the switches out from the rear of the steering wheel.

### Assembly Procedure

1. If the vehicle is equipped with cruise control, install the switches by pushing them in place from the front of the wheel.
2. Install the screws in the steering wheel shroud.