For 1990-2009 cars

The following table provides the description of the Regular Production Option (RPO) codes that are available on the vehicle. The vehicle's RPO list is printed on the Service Parts Identification Label.

RPO | Description
--- | ---
AG1 | Adjuster FRT ST Power, Multi-Directional, Drive
AH9 | Adjuster FRT ST Manual, 2 Way, Driver
AM1 | Control Seat, Manual Lumbar, Driver
AQ6 | Seat FRT, ADJ Back
ASF | Restraint, Roof Side, LH & RH, Inflatable
B58 | Covering Floor Mat, FRT and RR, Carpeted Insert
CF5 | Roof Sun, Glass, Sliding Electric
C60 | HVAC System Air Conditioner Front, Manual Control
C68 | HVAC System Air Conditioner FRT, Auto, Electronic Controls
C91 | Lamp INTR, Roof, Courtesy
C95 | Lamp INTR, Roof, Courtesy and Dual Reading
DA5 | Arm Rest RR Seat, Center
DC4 | Mirror I/S R/V Tilt, Dual Reading Lamps
DDCG9 | Mirror I/S R/V LT Sensitive, Compass, O/S TEMP Display VEH Communication SYS CONT, Dual Reading Lamps
DH6 | Mirror I/S FRT Van LH and RH, Sunshade, ILLUM
DL8 | Mirror O/S LH and RH, Remote Control, Electric, Heated
D22 | Mirror O/S LH and RH, Remote Control, Electric
D31 | Mirror I/S R/V Tilt
D34 | Mirror I/S FRT Van LH and RH, Sunshade, No Illumination
E3E | Handle O/S, L/Gate, R/CMPT, Chrome
FE9 | Certification Emission, Federal
FR3 | Ratio Transaxle Final Drive 3.69
FX2 | Ration Transaxle Final Drive 3.91
FX5 | Ration Transaxle Final Drive 4.45
JA7 | Handle Park BRK Release, Leather
JL9 | Brake System PWR, FRT and RR Disc, Antilock, FRT and RR WHL
JM4 | Brake System Power, Front Disc, RR Drum, Cast Iron, Antilock, FRT & RR WHL
J41 | Brake System PWR, FRT Disc, RR Drum, Cast Iron
J65 | Brake System PWR, FRT and RR Disc
KA1 | Heater Seat, FRT
K05 | Heater ENG Block
L61 | Engine Gas, 4 CYL, 2.2L, MFI, ALUM, DOHC
L81 | Engine Gas, 6 CYL, 3.0L, MFI, DOHC
MN4 | Transmission Auto 4 SPD, HMD, 4T45-E
MN5 | Merchandised TRANS MAN 4 SPD HMD, 4T45-E
MU3 | Transmission M AN 5 SPD, SAAB, 76.5 mm, 3.38 1st, 0.70 5th
NE1 | Certification Emission, Geographically Restricted Registration for Vehicles up to 14,000 lbs GVW (use 2003 MDL YR)
NP5 | Steering Wheel Leather Wrapped
NT9 | Emission System Federal, Tier 2 Phase-Out
NU4 | Emission System California LEV II Plus
N46 | Steering Wheel 4 Spokes
PG1 | Wheel 15 X 6, Steel
PY1 | Wheel 16 X 6.5, Aluminum, Chrome
QDJ | Tire All P215/55R16-91H BW R/PE ST TL AL3
QD2 | Wheel 16 x 6.5, Aluminum, 5 Spokes
QMC | Tire All P195/65R15-89T BW R/ST TL AL2
T96 | Lamp Fog, FRT
UB2 | Radio AM/FM Stereo, Seek/Scan, Auto REV Music Search CASS, Multiple CD, Auto Tone, Clock, ETR
UC1 | Speedometer INST, Miles
UE1 | Communication System Vehicle, G. P. S. 1
UP0 | Radio AM/FM Stereo, Seek/Scan, Auto REV Music Search CASS, CD, Auto Tone, Clock, ETR
UW5 | Speaker System 6, Base
U1C | Radio AM/FM Stereo, Seek/Scan, CD, Clock, ETR
U18 | Speedometer INST, KILO
U32 | Entertainment PKG Rear Seat, Player, DVD
U67 | Speaker System 7, QUAD FRT DR MTD, Dual RR MTD, Subwoof PKG Shelf, Amplifier, Bose
VK3 | License Plate Front FRT Mounting PKG
VY7 | Knob TRANS CONT Lever, Leather
V55 | Luggage Carrier Roof, Chrome
YF5 | Certification Emission, California
Z49 | Export Canadian Modify Mandatory Base Equipment