For 1990-2009 cars

Table 1: | Underhood Fuse Block Maxifuses
Table 2: | Underhood Fuse Block Minifuses -- Minifuses Circuit Feeds
Table 3: | Underhood Fuse Block Relays -- Relay Circuit Feeds
Table 4: | Left Instrument Panel Fuse Block Minifuses- Minifuses Circuit Feeds
Table 5: | Right Instrument Panel Fuse Block Minifuses -- Minifuses Circuit Feeds
Table 6: | Left Instrument Panel Fuse Block Relays Modules-- Relay Circuit Feeds
Table 7: | Right Instrument Panel Fuse Block Relays/Modules -- Relay Circuit Feeds

The wiring circuits in your vehicle are protected from short circuits by a combination of fuses. This greatly reduces the chance of fires caused by electrical problems.

There are three fuse blocks -- the "underhood fuse block," the "left instrument panel fuse block" and the "right instrument panel fuse block."

To identify and check fuses and relays, refer to the Fuse Usage Chart on the inside surface of the fuse panel door.

### Instrument Panel Fuse Block

The left instrument panel fuse block is located by driver's left leg.

The right instrument panel fuse block is located by the passenger's right leg.

Use a key or a coin to remove the fuse panel door and access the fuses and relays.

### Underhood Fuse Block

The underhood fuse block is located in the forward part of the engine compartment near the battery. When you replace a bad fuse, be sure to use one with the same rating.

Replace spare fuses as they are used as soon as you can. To identify and check fuses and relays, refer to the fuse and relay usage chart inside the fuse block cover.

To identify and check fuses and relays, refer to the fuse and relay usage chart inside the fuse block cover.

To remove a fuse, place the wide end of the fuse puller over the plastic end of the fuse. Squeeze the ends over the fuse and pull it out. A fuse puller is also located on the instrument panel junction block panel access door.

Look at the silver-colored band inside the fuse. If the band is broken or melted, replace the fuse. Be sure you replace a bad fuse with a new of the same amperage.

This chart lists the maxifuses and the minifuses they control and the following chart lists the systems they control.

#### Underhood Fuse Block Maxifuses

FUSE | COLOR (AMP) | SYSTEM
--- | --- | ---
IGN S 1/2 | Green (30) | Feeds ignition SW
IGN S 0/3/CR | Green (30) | Feeds ignition SW
COOL 1 | Green (30) | Feeds directly to cooling fan module
COOL 2 | Green (30) | Feeds directly to cooling fan module
ABS 1 | Green (30) | ABS power feed
ABS 2 | Green (30) | ABS power feed
Window/Sunroof | 30A Circuit Breaker | Feeds power window relay, sunroof (2.2L L4 [L61])
Window/Sunroof/Air | 30A Circuit Breaker | Feeds power window relay, sunroof and air pump relay (2.2L L4 [L61])
HVAC Blower | Amber (40) | Feeds Hi Blower

The following chart lists the minifuses, located in the underhood fuse block, and the circuits they control.

#### Underhood Fuse Block Minifuses -- Minifuses Circuit Feeds

FUSE | COLOR (AMP) | SYSTEM
--- | --- | ---
HORN | Red (10) | Horn
R HDLP | Red (10) | Right Headlamps
L HDLP | Red (10) | Left Headlamps
A/C | Red (10) | Air Conditioning System
LIGHTER | Yellow (20) | Cigar Lighter
AUX POWER | Yellow (20) | Power Outlet
RIGHT I/P BATT | Green (30) | Right Instrument Panel Fuse Block
CONTROLS B+ | Red (10) | Powertrain Control Module (2.2L L4), Engine Control Module (3.0L V6), Transaxle Control Module (3.0L V6)
BCM 2 | Yellow (20) | Body Control Module
BCM/ECM/CRUISE/ABS | Red (10) | Body Control Module, Engine Control Module, Cruise Control, ABS
EIS | Red (10) | Electronic Ignition System (2.2L L4)
IGN | Blue (15) | Ignition Coils (3.0L V6)
INJ | Red (10) | Fuel Injectors (2.2L L4)
BACK-UP/TURN | Red (10) | Backup Lamps, Coolant Level Switch
BRAKE | Red (10) | Brake Lamps
FUEL PUMP | Blue (15) | Fuel Pump Relay
IGN 0 | Red (10) | Park Neutral Position Switch, Powertrain Control Module
CRUISE SW | Gray (2) | Cruise Control Switch
CONTROLS IGN 1 | Red (10) | Cooling Fan Control Module, Powertrain Control Module, Transaxle (2.2L L4), Transaxle Control Module (3.0L V6)
IGN 1 | Red (10) | Instrument Cluster, Coolant Level Switch, Air Bag Electronic PRNDL321
BCM/CLUSTER | Blue (15) | Body Control Module, Instrument Cluster, Dimmer Switch
PARK LAMP | Red (10) | Front Park Lamps, Taillamps, Front Marker Lamps, Rear Marker Lamps, License Lamps, Radio Display Lights, I/P Cluster Backlighting, I/P Dimmer, Cigar Lighter Ring, Ashtray Light, PRNDL321 Light, HVAC Control Switch Backlighting
HAZARD | Blue (15) | Hazard Flasher, HBTT (Headlamp HI Beam Indicator), I/P Cluster
REAR DEFOG | Natural (25) | Rear Window Defogger
RADIO | Red (10) | Audio System, On Star (If Equipped)
CD/DLC | Blue (15) | Audio, Data Link Connector (DLC)
ING 3 | Red (10) | Cruise Clutch Switch, Emissions Controls, A/C Relay, Heated Oxygen Sensor, Vehicle Speed Signal Conditioner Module (2.2L L4 engine with manual transaxle and no ABS)
ENG CNTL 1 | Red (10) | 3.0L V6 Engine
ENG CNTL 2 | Red (10) | 3.0L V6 Engine
ENG CNTL 3 | Red (10) | 3.0L V6 Engine
COOLANT FLOW | Red (10) | Cooling Fan Module (3.0L V6 [L81])
AIR SOLENOID | Red (10) | Air Pump Solenoid (2.2L L4 [L61]) (California)
Device A/C Diode | - | A/C Diode (For Electrical System Protection)
OIL RESET | Oil Life Reset Switch | Oil Life Reset Switch

The following chart lists the relays, located in the underhood fuse block, and the systems they control.

#### Underhood Fuse Block Relays -- Relay Circuit Feeds

RELAY | SYSTEM
--- | ---
A/C | Air Conditioning System
DRL | Daytime Running Lamps
HORN | Horn
MAIN | 3.0L V6 Engine)
AIR PUMP | 2.2L L4 (L61) Engine
WIPER | Wiper System
FUEL PUMP | Fuel Pump System
REAR WIPER | Rear Wiper System (Wagon Only)

The following chart lists the minifuses, located in the left instrument panel fuse block, and the systems they control.

NOTE: Fuses are numbered in instrument panel fuse block. A label is provided on the fuse block access panel for fuse system description.

#### Left Instrument Panel Fuse Block Minifuses- Minifuses Circuit Feeds

FUSES | COLOR (AMP) | SYSTEM
--- | --- | ---
RADIO | Red (10) | Audio, On Star (If Equipped) Rear Seat DVD (Option)
WIPER | Natural (25) | Windshield Wipers and Washers (Front)
IGN 3 | Red (10) | Left Heated Seat Switch, Right Heated Seat Switch, Air Conditioning, Rear Defogger Relay
DEFOG LED | Red (10) | Rear Defog
BTSI/BCM/MIRROR | Red (10) | Brake Transaxle Shift Interlock, Body Control Module, Power Mirror
DIMMER | Red (10) | Dimmer Switch
Diode RR COMP LP | - | Trunk Compartment Lamp

The following chart lists the minifuses, located in the right instrument panel fuse block, and the systems they control.

#### Right Instrument Panel Fuse Block Minifuses -- Minifuses Circuit Feeds

FUSE | COLOR (AMP) | SYSTEM/FEED
--- | --- | ---
LOCKS | Blue (15) | Power Door Locks
BODY | Red (10) | Power Door Locks, Heated Mirror Relay, Liftgate Latch
POWER SEAT | Natural (25) | Power Seat
FOG LAMP | Red (10) | Fog Lamps
PREM AMP/MCS | Blue (15) | Premium Sound System Amplifier
HEATED SEATS | Yellow (20) | Seat Heater
RR WIPER/SUN ROOF | Yellow (20) | Rear Wiper/Washer (Wagon)

The following chart lists the relays and modules, located in the left instrument panel fuse block, and the systems they control.

#### Left Instrument Panel Fuse Block Relays Modules-- Relay Circuit Feeds

RELAY | SYSTEM
--- | ---
RR DEFOG | Rear Defogger
IGN 3 | Ignition Switch
PARKLAMP | Park Lamps
HEADLAMP | Headlapms

The following chart lists the relays and modules, located in the right instrument panel fuse block, and the systems they control.

#### Right Instrument Panel Fuse Block Relays/Modules -- Relay Circuit Feeds

RELAY | SYSTEM
--- | ---
POWER WINDOW | Power Windows, Power Sunroof
DRIVER DOOR UNLOCK RELAY | Driver Door Unlock
DOOR UNLOCK RELAY | Door Unlock
DOOR LOCK RELAY | Door Lock
HEATED MIRROR | Power Mirrors
FOG LAMP | Fog Lamps