For 1990-2009 cars

Important: The reverse synchronizer sleeve can only be placed on the reverse gear when the tall teeth on the sleeve are aligned with the deep tooth gaps in the gear.

Important: Lubricate all rotating parts and bearings with manual transaxle lubricant P/N 21018899 during assembly.

1. Install the reverse synchronizer sleeve to reverse gear. The chamfered edge of the sleeve goes down, towards reverse gear.
2. Install the reverse gear blocking ring with the spring on the reverse gear and synchronizer sleeve. Align the blocking ring lugs with gaps in the gear.
3. Install the reverse idler gear on the reverse gear blocking ring.
4. Install the reverse idler gear thrust bearing on the reverse idler shaft and install the shaft through the reverse idler and reverse gears.
5. Install the reverse gear washer.

Important: The reverse idler gear shaft lubrications hole, located on the opposite end of the shaft from the bracket, must be on the opposite side of the shaft from the reverse idler shaft support bracket hole when installing the bracket.

Important: Always use a new reverse idler gear shaft bracket.

Important: The tab on the reverse gear washer must fit between the lugs on the bottom of the shaft support bracket.

6. Install the new shaft support bracket with a press as shown. Make sure the bolt hole in the bracket aligns with the threaded shaft hole. Use a 17 mm socket to press on the bracket.
7. Measure the clearance between the reverse gear and reverse gear washer.

Specification
The tighten standard is 0.1-0.2 mm (0.004-0.0008 in).

Move the synchronizer sleeve up and down to check for proper operation.