For 1990-2009 cars

## Rear Bumper Fascia Emblem/Nameplate Replacement Solstice

Callout | Component Name
--- | ---
1 | Nameplate Assembly, Rear Bumper Fascia Tip

1. Clean the adhesive tape from the surface of the rear bumper fascia and dry thoroughly before applying the new emblem.
2. Peel the protective backing from the emblem and ensure no foreign matter or dirt comes in contact with the adhesive backing prior to installation.
3. Install the emblem and apply pressure to ensure full adhesion to the rear bumper fascia.

## Rear Bumper Fascia Emblem/Nameplate Replacement Solstice

Callout | Component Name
--- | ---
1 | Emblem Assembly, Rear Bumper Fascia Tip

1. Clean the adhesive tape from the surface of the rear bumper fascia and dry thoroughly before applying the new emblem.
2. Peel the protective backing from the emblem and ensure no foreign matter or dirt comes in contact with the adhesive backing prior to installation.
3. Install the emblem and apply pressure to ensure full adhesion to the rear bumper fascia.

## Rear Bumper Fascia Emblem/Nameplate Replacement Solstice

Callout | Component Name
--- | ---
1 | Nameplate Assembly, Rear Bumper Fascia Tip

1. Clean the adhesive tape from the surface of the rear bumper fascia and dry thoroughly before applying the new emblem.
2. Peel the protective backing from the emblem and ensure no foreign matter or dirt comes in contact with the adhesive backing prior to installation.
3. Install the emblem and apply pressure to ensure full adhesion to the rear bumper fascia.

## Rear Bumper Fascia Emblem/Nameplate Replacement SKY

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Using a J 25070 Heat Gun, warm the exterior bumper fascia to a minimum of 21°C (70°F) to assist with the adhesive tape removal and installation of the new rear compartment lid emblems.
2. Use a 50/50 mixture by volume of isopropyl alcohol and water in order to remove any adhesive tape residue from the rear bumper fascia after the emblems have been removed.

1 | Rear Compartment Lid Emblem Assembly (SATURN) Tip When removing the protective liners from the adhesive tape, be careful not to touch the tape with hands and do not allow the tape to come in contact with dirt or any foreign matter prior to adhesion.
2 | Rear Compartment Lid Emblem Assembly (SKY) Tip When removing the protective liners from the adhesive tape, be careful not to touch the tape with hands and do not allow the tape to come in contact with dirt or any foreign matter prior to adhesion.

## Rear Bumper Fascia Emblem/Nameplate Replacement Red Line

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Using a J 25070 Heat Gun, warm the exterior bumper fascia to a minimum of 21°C (70°F) to assist with the adhesive tape removal and installation of the new rear compartment lid emblems.
2. Use a 50/50 mixture by volume of isopropyl alcohol and water in order to remove any adhesive tape residue from the rear bumper fascia after the emblem has been removed.

1 | Rear Compartment Lid Emblem Assembly (Red Line)

#### Procedure

When removing the protective liners from the adhesive tape, be careful not to touch the tape with hands and do not allow the tape to come in contact with dirt or any foreign matter prior to adhesion.