For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the instrument panel (I/P) cluster trim plate. Refer to Instrument Cluster Trim Panel Replacement.
2. Remove the radio. Refer to Radio Replacement.
3. Remove the knee bolster panel. Refer to Knee Bolster Replacement.
4. Remove the I/P cup holder. Refer to Instrument Panel Cup Holder Replacement.

1 | Instrument Panel Extension Trim Plate Screw (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Instrument Panel Extension Trim Plate Assembly