For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: Refer to Fastener Caution in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications.

#### Preliminary Procedures

Open the folding top and stowage compartment lid.

1 | Folding Top Pivot Bracket Nuts (Qty: 3) Tip

• | Lift only the side of the folding top that the pivot bracket is to be replaced high enough to clear the adjusting pin.

• | Mark location relative to body of bracket.

• | Leave the alignment pin loose. Loose fit the top latch. Latch top to header. Check seal fit to door glass prior to tightening top alignment pin.

• | Adjust the folding top. Refer to Folding Top Adjustment.

Tighten
9 N·m (80 lb ft)

2 | Folding Top Pivot Bracket