For 1990-2009 cars

## Front Bumper Fascia Emblem Replacement Solstice

Callout | Component Name
--- | ---
1 | Emblem Assembly, Front Bumper Fascia Tip

1. Clean the adhesive tape from the surface of the front bumper fascia and dry thoroughly before applying the new emblem.
2. Peel the protective backing from the emblem and ensure no foreign matter or dirt comes in contact with the adhesive backing prior to installation.
3. Install the emblem and apply pressure to ensure full adhesion to the front bumper fascia.