For 1990-2009 cars

Caution: Refer to Fastener Caution in the Preface section.

1. Install new exhaust manifold studs and tighten to 10 N·m (89 lb in).
2. Install the exhaust manifold gasket.
3. Install the exhaust manifold to the cylinder head.
4. Install NEW exhaust manifold to cylinder head retaining nuts finger tight.
5. Tighten the NEW exhaust manifold to cylinder head retaining nuts in sequence. Tighten the nuts a second time to 14 N·m (124 lb in).
6. Coat the threads of the oxygen sensor with antiseize P/N 12397953 or equivalent.
7. Install the oxygen sensor and tighten to 42 N·m (31 lb ft).
8. Install the exhaust manifold heat shield.
9. Install the exhaust manifold heat shield bolts and tighten to 22 N·m (16 lb ft).