For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the radiator side air deflectors. Refer to Radiator Air Side Baffle and Deflector Replacement .

1 | Push Pin, Radiator Air Deflector - Front (Qty: 4)
2 | Bolt, Radiator Air Deflector - Front (Qty: 2) Tighten 9 N·m (80 lb in)
3 | Deflector Assembly, Radiator Air - Front