For 1990-2009 cars

#### Special Tools

J 44887 Oil Filter Wrench

For equivalent regional tools, refer to Special Tools

1. Install a new oil filter on the oil filter cap.
2. Lubricate the oil filter cap O-ring with 5W30 engine oil.

Caution: Refer to Fastener Caution in the Preface section.

3. Use the J 44887 Wrench to install the oil filter and cap. Tighten the oil filter and cap to 22 N·m (16 lb ft).