For 1990-2009 cars

## Heater Inlet Hose Replacement LE5

Callout | Component Name
--- | ---
Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedure

1. Drain the cooling system. Refer to Cooling System Draining and Filling .
2. Remove the air inlet grille panel. Refer to Air Inlet Grille Panel Replacement .

1 | Heater Inlet Hose Assembly

#### Procedure

Using J 38185 reposition the heater hose clamp.

## Heater Inlet Hose Replacement LNF

Callout | Component Name
--- | ---
Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedure

1. Drain the cooling system. Refer to Cooling System Draining and Filling .
2. Remove the air inlet grille panel. Refer to Air Inlet Grille Panel Replacement .

1 | Heater Inlet Hose Assembly

#### Procedure

Using J 38185 reposition the heater hose clamp.