For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
A/C Compressor to Block Bolt | 20 N·m | 15 lb ft
Balance Shaft Adjustable Chain Guide Bolt | 15 N·m | 11 lb ft
Balance Shaft Bearing Carrier to Block Bolt | 10 N·m | 89 lb in
Balance Shaft Fixed Chain Guide Bolt | 15 N·m | 11 lb ft
Balance Shaft Sprocket Bolt | 50 N·m | 37 lb ft
Block Core Plug | 40 N·m | 30 lb ft
Block Heater Bolt | 10 N·m | 89 lb in
Cam Cover to Cylinder Head Bolt | 10 N·m | 89 lb in
Cam Cover to Ground Cable Bolt | 10 N·m | 89 lb in
Cam Cover to Ground Cable Stud | 10 N·m | 89 lb in
Camshaft Cap Bolt | 10 N·m | 89 lb in
Camshaft Position Actuator Solenoid Valve Bolt | 10 N·m | 89 lb in
Camshaft Position Sensor Bolt | 10 N·m | 89 lb in
Camshaft Timing Chain Tensioner | 75 N·m | 55 lb ft
Chain Guide Plug | 90 N·m | 59 lb ft
Connecting Rod Bolt

- First Pass

25 N·m

18 lb ft

- Final Pass

100 degrees

Crankshaft Balancer Bolt

- First Pass

100 N·m

74 lb ft

- Final Pass

125 degrees

Crankshaft Bearings - Lower Crankcase to Block - Bedplate

- First Pass

20 N·m

15 lb ft

- Final Pass

70 degrees

Crankshaft Position Sensor Bolt | 10 N·m | 89 lb in
Cylinder Head Bolt

- First Pass

30 N·m

22 lb ft

- Final Pass

155 degrees

Cylinder Head Front Chaincase Bolt | 35 N·m | 26 lb ft
Cylinder Head Oil Gallery Plug | 35 N·m | 26 lb ft
Drive Belt Tensioner Bolt | 45 N·m | 33 lb ft
EGR Cover Bolt | 25 N·m | 18 lb ft
Engine Coolant Temperature Sensor | 20 N·m | 15 lb ft
Engine Lift Bracket Front Bolt | 25 N·m | 18 lb ft
Engine Lift Bracket Rear Bolt | 25 N·m | 18 lb ft
EVAP Canister Valve Bolt | 22 N·m | 16 lb ft
Exhaust Camshaft Position Actuator

- First Pass

30 N·m

22 lb ft

- Final Pass

100 degrees

Exhaust Manifold Pipe Flange Stud | 16 N·m | 12 lb ft
Exhaust Manifold to Cylinder Head Nut - 2 passes | 14 N·m | 124 lb in
Exhaust Manifold to Cylinder Head Stud | 10 N·m | 89 lb in
Flywheel Bolt - Automatic Transmission

- First Pass

53 N·m

39 lb ft

- Final Pass

25 degrees

Flywheel Bolt - Manual Transmission

- First Pass

53 N·m

39 lb ft

- Final Pass

25 degrees

Front Cover to Block Bolt | 25 N·m | 18 lb ft
Front Lift Bracket Bolt | 25 N·m | 18 lb ft
Fuel Pipe Bracket Bolt | 10 N·m | 89 lb in
Fuel Rail Bracket Stud | 10 N·m | 89 lb in
Generator to Block Bolt | 23 N·m | 17 lb ft
Heat Shield to Exhaust Manifold Bolt | 22 N·m | 16 lb ft
Ignition Coil Bolt | 10 N·m | 89 lb in
Intake Camshaft Position Actuator

- First Pass

30 N·m

22 lb ft

- Final Pass

100 degrees

Intake Camshaft Rear Cap Bolt | 25 N·m | 18 lb ft
Intake Manifold to Cylinder Head Bolt | 10 N·m | 89 lb in
Intake Manifold to Cylinder Head Nut | 10 N·m | 89 lb in
Intake Manifold to Cylinder Head Stud | 6 N·m | 53 lb in
Knock Sensor Bolt | 25 N·m | 18 lb ft
Lower Crankcase to Block Perimeter Bolt | 25 N·m | 18 lb ft
Oil Filter Housing Cover | 22 N·m | 16 lb ft
Oil Gallery Gerotor Cover - Rear Bolt | 6 N·m | 53 lb in
Oil Gallery Plug | 35 N·m | 26 lb ft
Oil Gallery Plug - Rear | 60 N·m | 44 lb ft
Oil Level Indicator Tube to Intake Manifold Bolt | 10 N·m | 89 lb in
Oil Pan Drain Plug | 25 N·m | 18 lb ft
Oil Pan to Block Bolts | 25 N·m | 18 lb ft
Oil Pressure Switch | 22 N·m | 16 lb ft
Oil Pump Cover Bolt | 6 N·m | 53 lb in
Oil Pump Pressure Relief Valve Plug | 40 N·m | 30 lb ft
Oxygen Sensor | 42 N·m | 31 lb ft
Piston Oil Squirter | 15 N·m | 11 lb ft
Power Steering Pump Bolt | 25 N·m | 18 lb ft
Spark Plug | 20 N·m | 15 lb ft
Starter Motor to Block Bolt | 53 N·m | 39 lb ft
Thermostat Housing to Block Bolts | 10 N·m | 89 lb in
Throttle Body Bolt | 10 N·m | 89 lb in
Throttle Body Nut | 10 N·m | 89 lb in
Throttle Body Stud | 6 N·m | 53 lb in
Timing Adjustable Chain Guide Bolt | 10 N·m | 89 lb in
Timing Chain Oil Nozzle Bolt | 10 N·m | 89 lb in
Timing Fixed Chain Guide Bolt | 15 N·m | 11 lb ft
Timing Upper Chain Guide Bolt | 10 N·m | 89 lb in
Vent Tube to Cylinder Head | 15 N·m | 11 lb ft
Water Jacket Drain Plug | 20 N·m | 15 lb ft
Water Pipe Support Bracket Bolt | 10 N·m | 89 lb in
Water Pump Access Cover Bolt | 7 N·m | 62 lb in
Water Pump/Balance Shaft Chain Tensioner Bolt | 10 N·m | 89 lb in
Water Pump Bolts | 25 N·m | 18 lb ft
Water Pump Sprocket Bolt | 10 N·m | 89 lb in