For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front wheelhouse liner. Refer to Front Wheelhouse Liner Replacement.

1 | Front Bumper Fascia Side Reinforcement Nuts (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
2 | Front Bumper Fascia Side Reinforcement Bolts (Qty: 2) Tighten 9 N·m (80 lb in)
3 | Front Bumper Fascia Side Reinforcement Tip Remove the screws from the end of the fascia and then remove the reinforcement.
4 | Front Bumper Fascia Brace Bolt (Qty: 1) Tighten 9 N·m (80 lb in)
5 | Front Bumper Fascia Brace
6 | Front Bumper Fascia Outer Support Bolt (Qty: 1) Tighten 9 N·m (80 lb in)
7 | Front Bumper Fascia Outer Support