For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear compartment trim. Refer to Rear Compartment Trim Panel Replacement .
2. Program the digital radio receiver after replacement. Refer to Control Module References .

1 | Digital Radio Receiver Bracket Nuts (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 10 N·m (89 lb in)
2 | Digital Radio Receiver Bracket Assembly
3 | Digital Radio Receiver Nuts (Qty: 3) Tighten 5 N·m (44 lb in)
4 | Digital Radio Receiver Assembly