For 1990-2009 cars

## Floor Panel Tunnel Panel Replacement - Front Manual Transmission

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Raise the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the exhaust system pipe. Refer to Muffler Replacement .

1 | Front Tunnel Panel Bolt (Qty: 9) Notice: Refer to Fastener Notice in the Preface section. Tighten 9 N·m (80 lb in)
2 | Front Tunnel Panel

## Floor Panel Tunnel Panel Replacement - Front Automatic Transmission

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Raise the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the exhaust system pipe. Refer to Muffler Replacement .

1 | Front Tunnel Panel Bolt (Qty: 9) Notice: Refer to Fastener Notice in the Preface section. Tighten 9 N·m (80 lb in)
2 | Front Tunnel Panel