For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Battery Cable Clip Stud | 10 N·m | 89 lb in
Battery Hold-Down Retainer Bolt | 25 N·m | 18 lb ft
Engine Harness Lead to Generator Nut | 20 N·m | 15 lb ft
Front Fender Rear Bracket Bolt | 20 N·m | 15 lb ft
Generator Bolt | 22 N·m | 16 lb ft
Negative Battery Cable Nut | 17 N·m | 13 lb ft
Negative Battery Cable Ground Bolt | 10 N·m | 89 lb in
Negative Battery Cable Ground Nut | 17 N·m | 13 lb ft
Positive Battery Cable Nutt | 17 N·m | 13 lb ft
Positive Cable to Starter Solenoid Nut | 10 N·m | 89 lb in
Starter Bolt | 40 N·m | 30 lb ft
Starter Solenoid S Terminal Nut | 3 N·m | 27 lb in