For 1990-2009 cars

## Rear Bumper Fascia Replacement Sky

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. For the coupe, remove the roof panel extension. Refer to Roof Panel Rear Extension Replacement.
2. Remove the tail lamp assembly. Refer to Tail Lamp Replacement.
3. Remove the right and left rear wheelhouse. Refer to Rear Wheelhouse Panel Liner Replacement.

1 | Rear Fascia Retainer (Qty: 4)
2 | Rear Fascia Screw (Qty: 7) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
3 | Rear Fascia Bracket Screw (Qty: 8)

#### Procedure

Reach between the fascia and the quarter panel to loosen the bolts.

Tighten
2 N·m (18 lb in)

4 | Rear Fascia Bracket Push-Pin (Qty: 2)
5 | Rear Fascia Tip Disconnect the lamp connectors.

## Rear Bumper Fascia Replacement Solstice

Callout | Component Name
--- | ---

#### Preliminary Procedure

• | Remove both fender liner sides. Refer to Rear Wheelhouse Panel Liner Replacement.

• | Remove the tail lamps. Refer to Tail Lamp Replacement.

• | Remove the high mount stop lamp. Refer to High Mount Stop Lamp Replacement.

• | Remove the backup lamps. Refer to Backup Lamp Replacement.

• | Remove the license lamp. Refer to Rear License Lamp Replacement.

1 | Rear Fascia Retainers (Qty: 6)
2 | Rear Fascia Retainers (Qty: 6)
3 | Rear Fascia Bolts (Qty: 6) Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (89 lb in)
4 | Rear Fascia Bolts (Qty: 8) Tighten 10 N·m (89 lb in)
5 | Rear Fascia