For 1990-2009 cars

# Rear Window Waterleak (Apply Sealer to Convertible Top)

Subject: | Rear Window Waterleak (Apply Sealer to Convertible Top)

Models: | 2006-2007 Pontiac Solstice

| 2007 Saturn Sky

This bulletin is being revised to add models and model years. Please discard Corporate Bulletin Number 06-08-57-002A (Section 08 - Body and Accessories).

### Condition

Some customers may comment on a waterleak from the rear window.

### Cause

This condition may be caused by the convertible top material separating from the back window.

### Correction

To repair this concern, clean the surfaces with *3M™ General Purpose Adhesive Cleaner. Then apply *3M™ Urethane (High Viscosity) Sealer, P/N 08609, between the two surfaces and let cure following manufacturer's recommendations.

*We believe this source and their products to be reliable. There may be additional manufacturers of such products. General Motors does not endorse, indicate any preference for or assume any responsibility for the products from this firm or for any such items which may be available from other sources.

### Warranty Information

For vehicles repaired under warranty, use:

Labor Operation | Description | Labor Time
--- | --- | ---
B9781* | Reseal Back Glass | 0.5 hr
*This is a unique labor operation for bulletin use only. It will not be published in the Labor Time Guide.