For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the underhood bussed electrical center (BEC) bracket bolts and reposition the bracket and electrical center out of the way.
3. Remove the negative battery cable ground nut (4) at the side rail stud.
4. Remove the negative battery cable terminal (3) from the stud.
5. Remove the negative battery cable ground terminal bolt.
6. Remove the negative battery cable ground terminal and engine harness ground terminal from the cylinder head.
7. Remove the negative battery cable ground nut (1) at the bussed electrical center (BEC) stud.
8. Remove the negative battery cable terminal from the BEC stud.
9. Remove the negative battery cable clips (4) from the wheelhouse liner.
10. Remove the battery cable clip bolt (3).
11. Remove the negative battery cable out through the engine wiring harness junction block bracket.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the negative battery cable. Route the cable through the engine wiring harness junction block bracket to battery, main side rail, and BEC.
2. Install the battery cable clip bolt (3).

Tighten
Tighten the bolt to 10 N·m (89 lb in).

3. Install the negative battery cable clips (4) to the wheelhouse liner.
4. Install the negative battery cable terminal from the BEC stud.
5. Install the negative battery cable ground nut (1) at the BEC stud.

Tighten
Tighten the nut to 10 N·m (89 lb in).

6. Position the engine harness ground terminal behind the negative battery cable terminal and position against the cylinder head.
7. Install the negative battery cable ground bolt.

Tighten
Tighten the bolt to 10 N·m (89 lb in).

8. Install the negative battery cable terminal (3) to the stud.
9. Install the negative battery cable ground nut (4) at the side rail stud.

Tighten
Tighten the nut to 10 N·m (89 lb in).

10. position the underhood BEC bracket and electrical center and install the bolts.

Tighten
Tighten the bolts to 25 N·m (18 lb ft).

11. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.