For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the top from the vehicle. Refer to Folding Top Replacement .

1 | Folding Clock Spring Rivet Tip Drill out the rivet.
2 | Outboard Spring Tip The spring has minimal tension when the top is in the stowed position.
3 | Inboard Spring Tip

• | The inboard spring has minimal tension when the top is in the raised position.

• | The inboard spring is larger in diameter than the outboard spring.

• | The inboard/outboard springs have opposite winding.