For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: Refer to Fastener Caution in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications.

#### Preliminary Procedures

Open the folding top, position the No. 1 bow in the upright position.

1 | Screws, Retainer Folding Top Cover No. 1 Bow (Qty: 10) Tip The retainer is located on the front inside edge of the folding top. Tighten 2 N·m (18 lb in)
2 | Retainer, Folding Top Cover No. 1 Bow